**DP5051TM6S21016 –***Adjustable Doc & Pin – Heavy-Duty*

**Product Specifications**

**Specification Summary:**Adjustable Doc & Pin – Heavy-Duty - Taper Face Fitting (Single Connection): Provide Type 316 finished stainless steel with black gaskets and ferrule bushing able to accommodate 12 mm to 21.5 mm glass thickness. Distance between glass and centre of pin mounting surface is adjustable, between 71 mm and 83 mm. Loading Capacity: 3.5kN﻿. Permitted Product: “Model DP5051TM6S21016” by Stella Glass Hardware; [www.stellaglasshardware.com](http://www.stellaglasshardware.com).

**Specification Details:**

* Division:
  + Found in Divisions 05 & 08
* Materials:
  + Steel: Grade 316 stainless steel
  + Finish: No. 4, 320 grit
  + Gaskets: Material based on high-quality aramid fibers and special functional fillers bonded with NBR, sulfur-free, solvent-free
  + Ferrule Bushing: Acetal delrin
* Mount Type: Side mount
* Mounting Structure: Glass, concrete, steel or wood
  + Substrate thickness: 10mm to 16mm [3/8" to 5/8"]
* Loading Capability: 3.5kN
* LEED Standards:
  + Stainless Steel (primary material) - >45% pre-/95% post- consumer recycled content by weight
* Compliances/Standard: Project specific
* Warranty: 2-year limited warranty\* (can be project specific)