**SS202FTNHH6S013 –***Heavy-Duty Two Arm (Face-Mount) Spider*

**Product Specifications**

**Specification Summary:**Heavy-Duty Straight Line Two Arm (Face-Mount) Spider Fitting (SS20): Provide Type 316 finished stainless steel with hex bolt M16 x 50, comes with washers (2) and spring washer. Loading capability: lateral load 1.5kN (per leg), tensile load 3.7kN; for compression load, refer to loading capacity of the glass bolt chosen. Need glass bolts to affix spider to glass. Permitted Product: “Model SS202FTNHH6S013” by Stella Glass Hardware; [www.stellaglasshardware.com](http://www.stellaglasshardware.com).

**Specification Details:**

* Division:
	+ 08 88 00: Special Function Glazing
* Materials:
	+ Steel: Grade 316 stainless steel
	+ Finish: No. 4, 320 grit
* Mount Type: Face-mount
* Mount Structure: Concrete, steel or wood
	+ Mounting Substrate Thickness: 6 to 13mm [1/4" to 1/2"]
* Loading Capability: Lateral load 1.5kN (per leg), Tensile load 3.7kN
(for compression load, refer to loading capacity of the Stella Glass Bolt chosen)
* LEED Standards:
	+ Stainless Steel (primary material) - >45% pre-/95% post- consumer recycled content by weight
* Compliances/Standard: Project specific
* Warranty: 2-year limited warranty\* (can be project specific)